The first step in interacting with a BLE device is connecting to it. More specifically, connecting to the GATT server on the device. To connect to a GATT server on a BLE device, use the[`connectGatt()`](https://developer.android.com/reference/android/bluetooth/BluetoothDevice#connectGatt(android.content.Context,%20boolean,%20android.bluetooth.BluetoothGattCallback))method. This method takes three parameters: a[`Context`](https://developer.android.com/reference/android/content/Context)object,`autoConnect`(a boolean indicating whether to automatically connect to the BLE device as soon as it becomes available), and a reference to a[`BluetoothGattCallback`](https://developer.android.com/reference/android/bluetooth/BluetoothGattCallback):  

### Kotlin

```kotlin
var bluetoothGatt: BluetoothGatt? = null
...

bluetoothGatt = device.connectGatt(this, false, gattCallback)
```

### Java

```java
bluetoothGatt = device.connectGatt(this, false, gattCallback);
```

This connects to the GATT server hosted by the BLE device, and returns a[`BluetoothGatt`](https://developer.android.com/reference/android/bluetooth/BluetoothGatt)instance, which you can then use to conduct GATT client operations. The caller (the Android app) is the GATT client. The`BluetoothGattCallback`is used to deliver results to the client, such as connection status, as well as any further GATT client operations.

## Set up a bound service

In the following example, the BLE app provides an activity (`DeviceControlActivity`) to connect to Bluetooth devices, display device data, and display the GATT services and characteristics supported by the device. Based on user input, this activity communicates with a[`Service`](https://developer.android.com/reference/android/app/Service)called`BluetoothLeService`, which interacts with the BLE device via the BLE API. The communication is performed using a[bound service](https://developer.android.com/guide/components/bound-services)which allows the activity to connect to the`BluetoothLeService`and call functions to connect to the devices. The`BluetoothLeService`needs a[`Binder`](https://developer.android.com/reference/android/os/Binder)implementation that provides access to the service for the activity.  

### Kotlin

```kotlin
class BluetoothLeService : Service() {

    private val binder = LocalBinder()

    override fun onBind(intent: Intent): IBinder? {
        return binder
    }

    inner class LocalBinder : Binder() {
        fun getService() : BluetoothLeService {
            return this@BluetoothLeService
        }
    }
}
```

### Java

```java
class BluetoothLeService extends Service {

    private Binder binder = new LocalBinder();

    @Nullable
    @Override
    public IBinder onBind(Intent intent) {
        return binder;
    }

    class LocalBinder extends Binder {
        public BluetoothLeService getService() {
            return BluetoothLeService.this;
        }
    }
}
```

The activity can start the service using[`bindService()`](https://developer.android.com/reference/android/content/Context#bindService(android.content.Intent,%20android.content.ServiceConnection,%20int)), passing in an[`Intent`](https://developer.android.com/reference/android/content/Intent)to start the service, a[`ServiceConnection`](https://developer.android.com/reference/android/content/ServiceConnection)implementation to listen for the connection and disconnection events, and a flag to specify additional connection options.  

### Kotlin

```kotlin
class DeviceControlActivity : AppCompatActivity() {

    private var bluetoothService : BluetoothLeService? = null

    // Code to manage Service lifecycle.
    private val serviceConnection: ServiceConnection = object : ServiceConnection {
        override fun onServiceConnected(
            componentName: ComponentName,
            service: IBinder
        ) {
            bluetoothService = (service as LocalBinder).getService()
            bluetoothService?.let { bluetooth ->
                // call functions on service to check connection and connect to devices
            }
        }

        override fun onServiceDisconnected(componentName: ComponentName) {
            bluetoothService = null
        }
    }

    override fun onCreate(savedInstanceState: Bundle?) {
        super.onCreate(savedInstanceState)
        setContentView(R.layout.gatt_services_characteristics)

        val gattServiceIntent = Intent(this, BluetoothLeService::class.java)
        bindService(gattServiceIntent, serviceConnection, Context.BIND_AUTO_CREATE)
    }
}
```

### Java

```java
class DeviceControlActivity extends AppCompatActivity {

    private BluetoothLeService bluetoothService;

    private ServiceConnection serviceConnection = new ServiceConnection() {
        @Override
        public void onServiceConnected(ComponentName name, IBinder service) {
            bluetoothService = ((LocalBinder) service).getService();
            if (bluetoothService != null) {
                // call functions on service to check connection and connect to devices
            }
        }

        @Override
        public void onServiceDisconnected(ComponentName name) {
            bluetoothService = null;
        }
    };

    @Override
    protected void onCreate(@Nullable Bundle savedInstanceState) {
        super.onCreate(savedInstanceState);
        setContentView(R.layout.gatt_services_characteristics);

        Intent gattServiceIntent = new Intent(this, BluetoothLeService.class);
        bindService(gattServiceIntent, serviceConnection, Context.BIND_AUTO_CREATE);
    }
}
```

## Set up the BluetoothAdapter

Once the service is bound to, it needs to access the[`BluetoothAdapter`](https://developer.android.com/reference/android/bluetooth/BluetoothAdapter). It should check that the adapter is available on the device. Read[Set up Bluetooth](https://developer.android.com/develop/connectivity/bluetooth/setup)for more information on the`BluetoothAdapter`. The following example wraps this setup code in an`initialize()`function that returns a`Boolean`value indicating success.  

### Kotlin

```kotlin
private const val TAG = "BluetoothLeService"

class BluetoothLeService : Service() {

    private var bluetoothAdapter: BluetoothAdapter? = null

    fun initialize(): Boolean {
        bluetoothAdapter = BluetoothAdapter.getDefaultAdapter()
        if (bluetoothAdapter == null) {
            Log.e(TAG, "Unable to obtain a BluetoothAdapter.")
            return false
        }
        return true
    }

    ...
}
```

### Java

```java
class BluetoothLeService extends Service {

    public static final String TAG = "BluetoothLeService";

    private BluetoothAdapter bluetoothAdapter;

    public boolean initialize() {
        bluetoothAdapter = BluetoothAdapter.getDefaultAdapter();
        if (bluetoothAdapter == null) {
            Log.e(TAG, "Unable to obtain a BluetoothAdapter.");
            return false;
        }
        return true;
    }

    ...
}
```

The activity calls this function within its`ServiceConnection`implementation. Handling a false return value from the`initialize()`function depends on your application. You could show an error message to the user indicating that the current device does not support the Bluetooth operation or disable any features that require Bluetooth to work. In the following example,[`finish()`](https://developer.android.com/reference/android/app/Activity#finish())is called on the activity to send the user back to the previous screen.  

### Kotlin

```kotlin
class DeviceControlActivity : AppCompatActivity() {

    // Code to manage Service lifecycle.
    private val serviceConnection: ServiceConnection = object : ServiceConnection {
        override fun onServiceConnected(
            componentName: ComponentName,
            service: IBinder
        ) {
            bluetoothService = (service as LocalBinder).getService()
            bluetoothService?.let { bluetooth ->
                if (!bluetooth.initialize()) {
                    Log.e(TAG, "Unable to initialize Bluetooth")
                    finish()
                }
                // perform device connection
            }
        }

        override fun onServiceDisconnected(componentName: ComponentName) {
            bluetoothService = null
        }
    }

    ...
}
```

### Java

```java
class DeviceControlsActivity extends AppCompatActivity {

    private ServiceConnection serviceConnection = new ServiceConnection() {
        @Override
        public void onServiceConnected(ComponentName name, IBinder service) {
            bluetoothService = ((LocalBinder) service).getService();
            if (bluetoothService != null) {
                if (!bluetoothService.initialize()) {
                    Log.e(TAG, "Unable to initialize Bluetooth");
                    finish();
                }
                // perform device connection
            }
        }

        @Override
        public void onServiceDisconnected(ComponentName name) {
            bluetoothService = null;
        }
    };

    ...
}
```

## Connect to a device

Once the`BluetoothLeService`instance is initialized, it can connect to the BLE device. The activity needs to send the device address to the service so it can initiate the connection. The service will first call[`getRemoteDevice()`](https://developer.android.com/reference/android/bluetooth/BluetoothAdapter#getRemoteDevice(java.lang.String))on the`BluetoothAdapter`to access the device. If the adapter is unable to find a device with that address,`getRemoteDevice()`throws an[`IllegalArgumentException`](https://developer.android.com/reference/java/lang/IllegalArgumentException).  

### Kotlin

```kotlin
fun connect(address: String): Boolean {
    bluetoothAdapter?.let { adapter ->
        try {
            val device = adapter.getRemoteDevice(address)
        } catch (exception: IllegalArgumentException) {
            Log.w(TAG, "Device not found with provided address.")
            return false
        }
    // connect to the GATT server on the device
    } ?: run {
        Log.w(TAG, "BluetoothAdapter not initialized")
        return false
    }
}
```

### Java

```java
public boolean connect(final String address) {
    if (bluetoothAdapter == null || address == null) {
        Log.w(TAG, "BluetoothAdapter not initialized or unspecified address.");
        return false;
    }

    try {
        final BluetoothDevice device = bluetoothAdapter.getRemoteDevice(address);
    } catch (IllegalArgumentException exception) {
        Log.w(TAG, "Device not found with provided address.");
        return false;
    }
    // connect to the GATT server on the device
}
```

The`DeviceControlActivity`calls this`connect()`function once the service is initialized. The activity needs to pass in the address of the BLE device. In the following example, the device address is passed to the activity as an intent extra.  

### Kotlin

```kotlin
// Code to manage Service lifecycle.
private val serviceConnection: ServiceConnection = object : ServiceConnection {
    override fun onServiceConnected(
    componentName: ComponentName,
    service: IBinder
    ) {
        bluetoothService = (service as LocalBinder).getService()
        bluetoothService?.let { bluetooth ->
            if (!bluetooth.initialize()) {
                Log.e(TAG, "Unable to initialize Bluetooth")
                finish()
            }
            // perform device connection
            bluetooth.connect(deviceAddress)
        }
    }

    override fun onServiceDisconnected(componentName: ComponentName) {
        bluetoothService = null
    }
}
```

### Java

```java
private ServiceConnection serviceConnection = new ServiceConnection() {
    @Override
    public void onServiceConnected(ComponentName name, IBinder service) {
        bluetoothService = ((LocalBinder) service).getService();
        if (bluetoothService != null) {
            if (!bluetoothService.initialize()) {
                Log.e(TAG, "Unable to initialize Bluetooth");
                finish();
            }
            // perform device connection
            bluetoothService.connect(deviceAddress);
        }
    }

    @Override
    public void onServiceDisconnected(ComponentName name) {
        bluetoothService = null;
    }
};
```

## Declare GATT callback

Once the activity tells the service which device to connect to and the service connects to the device, the service needs to connect to the GATT server on the BLE device. This connection requires a`BluetoothGattCallback`to receive notifications about the connection state, service discovery, characteristic reads, and characteristic notifications.

This topic focuses on the connection state notifications. See[Transfer BLE data](https://developer.android.com/develop/connectivity/bluetooth/ble/transfer-ble-data)for how to perform service discovery, characteristic reads, and request characteristic notifications.

The[`onConnectionStateChange()`](https://developer.android.com/reference/android/bluetooth/BluetoothGattCallback#onConnectionStateChange(android.bluetooth.BluetoothGatt,%20int,%20int))function is triggered when the connection to the device's GATT server changes. In the following example, the callback is defined in the`Service`class so it can be used with the[`BluetoothDevice`](https://developer.android.com/reference/android/bluetooth/BluetoothDevice)once the service connects to it.  

### Kotlin

```kotlin
private val bluetoothGattCallback = object : BluetoothGattCallback() {
    override fun onConnectionStateChange(gatt: BluetoothGatt?, status: Int, newState: Int) {
        if (newState == BluetoothProfile.STATE_CONNECTED) {
            // successfully connected to the GATT Server
        } else if (newState == BluetoothProfile.STATE_DISCONNECTED) {
            // disconnected from the GATT Server
        }
    }
}
```

### Java

```java
private final BluetoothGattCallback bluetoothGattCallback = new BluetoothGattCallback() {
    @Override
    public void onConnectionStateChange(BluetoothGatt gatt, int status, int newState) {
        if (newState == BluetoothProfile.STATE_CONNECTED) {
            // successfully connected to the GATT Server
        } else if (newState == BluetoothProfile.STATE_DISCONNECTED) {
            // disconnected from the GATT Server
        }
    }
};
```

## Connect to GATT service

Once the`BluetoothGattCallback`is declared, the service can use the`BluetoothDevice`object from the`connect()`function to connect to the GATT service on the device.

The[`connectGatt()`](https://developer.android.com/reference/android/bluetooth/BluetoothDevice#connectGatt(android.content.Context,%20boolean,%20android.bluetooth.BluetoothGattCallback))function is used. This requires a`Context`object, an`autoConnect`boolean flag, and the`BluetoothGattCallback`. In this example, the app is directly connecting to the BLE device, so`false`is passed for`autoConnect`.

A`BluetoothGatt`property is also added. This allows the service to[close the connection](https://developer.android.com/reference/android/bluetooth/BluetoothGatt#close())when it is no longer needed.  

### Kotlin

```kotlin
class BluetoothLeService : Service() {

...

    private var bluetoothGatt: BluetoothGatt? = null

    ...

    fun connect(address: String): Boolean {
        bluetoothAdapter?.let { adapter ->
            try {
                val device = adapter.getRemoteDevice(address)
                // connect to the GATT server on the device
                bluetoothGatt = device.connectGatt(this, false, bluetoothGattCallback)
                return true
            } catch (exception: IllegalArgumentException) {
                Log.w(TAG, "Device not found with provided address.  Unable to connect.")
                return false
            }
        } ?: run {
            Log.w(TAG, "BluetoothAdapter not initialized")
            return false
        }
    }
}
```

### Java

```java
class BluetoothLeService extends Service {

...

    private BluetoothGatt bluetoothGatt;

    ...

    public boolean connect(final String address) {
        if (bluetoothAdapter == null || address == null) {
            Log.w(TAG, "BluetoothAdapter not initialized or unspecified address.");
            return false;
        }
        try {
            final BluetoothDevice device = bluetoothAdapter.getRemoteDevice(address);
            // connect to the GATT server on the device
            bluetoothGatt = device.connectGatt(this, false, bluetoothGattCallback);
            return true;
        } catch (IllegalArgumentException exception) {
            Log.w(TAG, "Device not found with provided address.  Unable to connect.");
            return false;
        }
    }
}
```

## Broadcast updates

When the server connects or disconnects from the GATT server, it needs to notify the activity of the new state. There are several ways to accomplish this. The following example uses[broadcasts](https://developer.android.com/guide/components/broadcasts)to send the information from the service to activity.

The service declares a function to broadcast the new state. This function takes in an action string which is passed to an`Intent`object before being broadcast to the system.  

### Kotlin

```kotlin
private fun broadcastUpdate(action: String) {
    val intent = Intent(action)
    sendBroadcast(intent)
}
```

### Java

```java
private void broadcastUpdate(final String action) {
    final Intent intent = new Intent(action);
    sendBroadcast(intent);
}
```

Once the broadcast function is in place, it is used within the`BluetoothGattCallback`to send information about the connection state with the GATT server. Constants and the service's current connection state are declared in the service representing the`Intent`actions.  

### Kotlin

```kotlin
class BluetoothLeService : Service() {

    private var connectionState = STATE_DISCONNECTED

    private val bluetoothGattCallback: BluetoothGattCallback = object : BluetoothGattCallback() {
        override fun onConnectionStateChange(gatt: BluetoothGatt, status: Int, newState: Int) {
            if (newState == BluetoothProfile.STATE_CONNECTED) {
                // successfully connected to the GATT Server
                connectionState = STATE_CONNECTED
                broadcastUpdate(ACTION_GATT_CONNECTED)
            } else if (newState == BluetoothProfile.STATE_DISCONNECTED) {
                // disconnected from the GATT Server
                connectionState = STATE_DISCONNECTED
                broadcastUpdate(ACTION_GATT_DISCONNECTED)
            }
        }
    }

    ...

    companion object {
        const val ACTION_GATT_CONNECTED =
            "com.example.bluetooth.le.ACTION_GATT_CONNECTED"
        const val ACTION_GATT_DISCONNECTED =
            "com.example.bluetooth.le.ACTION_GATT_DISCONNECTED"

        private const val STATE_DISCONNECTED = 0
        private const val STATE_CONNECTED = 2

    }
}
```

### Java

```java
class BluetoothLeService extends Service {

    public final static String ACTION_GATT_CONNECTED =
            "com.example.bluetooth.le.ACTION_GATT_CONNECTED";
    public final static String ACTION_GATT_DISCONNECTED =
            "com.example.bluetooth.le.ACTION_GATT_DISCONNECTED";

    private static final int STATE_DISCONNECTED = 0;
    private static final int STATE_CONNECTED = 2;

    private int connectionState;
    ...

    private final BluetoothGattCallback bluetoothGattCallback = new BluetoothGattCallback() {
        @Override
        public void onConnectionStateChange(BluetoothGatt gatt, int status, int newState) {
            if (newState == BluetoothProfile.STATE_CONNECTED) {
                // successfully connected to the GATT Server
                connectionState = STATE_CONNECTED;
                broadcastUpdate(ACTION_GATT_CONNECTED);
            } else if (newState == BluetoothProfile.STATE_DISCONNECTED) {
                // disconnected from the GATT Server
                connectionState = STATE_DISCONNECTED;
                broadcastUpdate(ACTION_GATT_DISCONNECTED);
            }
        }
    };

    ...
}
```

## Listen for updates in activity

Once the service broadcasts the connection updates, the activity needs to implement a[`BroadcastReceiver`](https://developer.android.com/reference/android/content/BroadcastReceiver). Register this receiver when setting up the activity, and unregister it when the activity is leaving the screen. By listening for the events from the service, the activity is able to update the user interface based on the current connection state with the BLE device.  

### Kotlin

```kotlin
class DeviceControlActivity : AppCompatActivity() {

...

    private val gattUpdateReceiver: BroadcastReceiver = object : BroadcastReceiver() {
        override fun onReceive(context: Context, intent: Intent) {
            when (intent.action) {
                BluetoothLeService.ACTION_GATT_CONNECTED -> {
                    connected = true
                    updateConnectionState(R.string.connected)
                }
                BluetoothLeService.ACTION_GATT_DISCONNECTED -> {
                    connected = false
                    updateConnectionState(R.string.disconnected)
                }
            }
        }
    }

    override fun onResume() {
        super.onResume()
        registerReceiver(gattUpdateReceiver, makeGattUpdateIntentFilter())
        if (bluetoothService != null) {
            val result = bluetoothService!!.connect(deviceAddress)
            Log.d(DeviceControlsActivity.TAG, "Connect request result=$result")
        }
    }

    override fun onPause() {
        super.onPause()
        unregisterReceiver(gattUpdateReceiver)
    }

    private fun makeGattUpdateIntentFilter(): IntentFilter? {
        return IntentFilter().apply {
            addAction(BluetoothLeService.ACTION_GATT_CONNECTED)
            addAction(BluetoothLeService.ACTION_GATT_DISCONNECTED)
        }
    }
}
```

### Java

```java
class DeviceControlsActivity extends AppCompatActivity {

...

    private final BroadcastReceiver gattUpdateReceiver = new BroadcastReceiver() {
        @Override
        public void onReceive(Context context, Intent intent) {
            final String action = intent.getAction();
            if (BluetoothLeService.ACTION_GATT_CONNECTED.equals(action)) {
                connected = true;
                updateConnectionState(R.string.connected);
            } else if (BluetoothLeService.ACTION_GATT_DISCONNECTED.equals(action)) {
                connected = false;
                updateConnectionState(R.string.disconnected);
            }
        }
    };

    @Override
    protected void onResume() {
        super.onResume();

        registerReceiver(gattUpdateReceiver, makeGattUpdateIntentFilter());
        if (bluetoothService != null) {
            final boolean result = bluetoothService.connect(deviceAddress);
            Log.d(TAG, "Connect request result=" + result);
        }
    }

    @Override
    protected void onPause() {
        super.onPause();
        unregisterReceiver(gattUpdateReceiver);
    }

    private static IntentFilter makeGattUpdateIntentFilter() {
        final IntentFilter intentFilter = new IntentFilter();
        intentFilter.addAction(BluetoothLeService.ACTION_GATT_CONNECTED);
        intentFilter.addAction(BluetoothLeService.ACTION_GATT_DISCONNECTED);
        return intentFilter;
    }
}
```

In[Transfer BLE data](https://developer.android.com/develop/connectivity/bluetooth/ble/transfer-ble-data), the`BroadcastReceiver`is also used to communicate the service discovery as well as the characteristic data from the device.

## Close GATT connection

One important step when dealing with Bluetooth connections is to close the connection when you are finished with it. To do this, call the`close()`function on the`BluetoothGatt`object. In the following example, the service holds the reference to the`BluetoothGatt`. When the activity unbinds from the service, the connection is closed to avoid draining the device battery.  

### Kotlin

```kotlin
class BluetoothLeService : Service() {

...

    override fun onUnbind(intent: Intent?): Boolean {
        close()
        return super.onUnbind(intent)
    }

    private fun close() {
        bluetoothGatt?.let { gatt ->
            gatt.close()
            bluetoothGatt = null
        }
    }
}
```

### Java

```java
class BluetoothLeService extends Service {

...

      @Override
      public boolean onUnbind(Intent intent) {
          close();
          return super.onUnbind(intent);
      }

      private void close() {
          if (bluetoothGatt == null) {
              Return;
          }
          bluetoothGatt.close();
          bluetoothGatt = null;
      }
}
```